# Dune HD Z-Wave Plugin

*dune\_plugin\_zwave\_controller.smp875x.2017\_10\_20*

This plugin is made for all Dune HD models in the 4K series (models with the Sigma SMP875x chipset). It is a Z-Wave controller plugin that adds the ability to use the Dune players as a Z-Wave controller. Please note that it is necessary for this plugin to have an internal Z-Wave module or to have a Z-Wave.Me UZB stick connected to one of the USB ports.

## Installation Instructions

1. Place the “dune\_plugin\_zwave\_controller.smp875x.2017\_10\_20.zip” file on a USB stick and plug the USB stick into one of the USB ports of your Dune HD player.
2. Open the Dune file browser and navigate to the directory of the USB stick.
3. Select the “dune\_plugin\_zwave\_controller.smp875x.2017\_10\_20.zip” file and press the “Enter” button on your remote.
4. The player will start loading. After a while a message will pop up that the plugin is successfully installed, now press “Launch”.
5. The plugin is now successfully installed and running!

For further instructions on the usage of the plugin, open the plugin from the Dune’s application menu or visit this page:

<http://dune-hd.com/firmware/z-wave/>